Creating accurate ortho-mosaic image maps from large columes of aerial imagery using traditional methods is a time-consuming task, even when completed using high-end hardware and software systems. This article challenges the traditional methods and requirements. Over one weekend we push a laptop computer, configured with automated production software, to the edge by attempting to process 4,000 large format UltraCamX aerial photos, from elevation model creation to the final mosaic.